<?xml version="1.0" encoding="utf-8"?>
<!-- (c) Copyright IBM Corp. 2004, 2005 All Rights Reserved. -->

<!DOCTYPE task PUBLIC "-//OASIS//DTD DITA Task//EN"
 "../../dtd/task.dtd">
<task id="insertdrive" xml:lang="en-us">
<title>Attach the drive to the system</title>
<shortdesc>The drive needs to be attached to power cables and other cables
inside the computer.</shortdesc>
<prolog><metadata>
<keywords><indexterm>hard drive</indexterm></keywords>
</metadata></prolog>
<taskbody>
<prereq><note type="caution">You must be grounded before doing this.</note></prereq>
<steps>
<step><cmd>Find an empty bay for your drive.</cmd></step>
<step><cmd>Remove the drive from its electrostatic bag.</cmd></step>
<step><cmd>Screw the drive in to the frame.</cmd></step>
<step><cmd>Attach the multi-colored power cord to the drive.</cmd></step>
<step><cmd>Attach the cable that connects your hard drive to the motherboard.</cmd>
</step>
</steps>
</taskbody>
</task>
